READ ME:

EC 413 Lab 3 – Brendan Shortall U71270986

Predicted gate delay:

64b RCA: 128 (64 FA\*2)

64b Carry Select: 8 (4 stages)

Graphical user interface

Description automatically generated64bit RCA with delay. Delay = 114.

Graphical user interface

Description automatically generated 64bit RCA no delay

Graphical user interface

Description automatically generated64bit Carry select adder no delay

Graphical user interface

Description automatically generated64 bit carry select adder with delay, delay = 8.